AceWire 0.3.2 Unified interface for selecting different I2C implementations on Arduino platforms

ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > Member List

This is the complete list of members for ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS >, including all inherited members.

begin() const | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
beginTransmission(uint8_t addr) const | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
end() const | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
endTransmission(bool sendStop=true) const | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
operator=(const SimpleWireFastInterface &)=default (defined in ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS >) | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > |
read() | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
requestFrom(uint8_t addr, uint8_t quantity, bool sendStop=true) | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline
SimpleWireFastInterface()=default | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | explicit
SimpleWireFastInterface(const SimpleWireFastInterface &)=default (defined in ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS >) | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > |
write(uint8_t data) const | ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > | inline