AceWire 0.3.2 Unified interface for selecting different I2C implementations on Arduino platforms

Here is a list of all documented class members with links to the class documentation for each member:

- begin() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- beginTransmission() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- end() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- endTransmission() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- read() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- requestFrom() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >
- SimpleWireFastInterface() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS >
- SimpleWireInterface() : ace_wire::SimpleWireInterface
- TwoWireInterface() : ace_wire::TwoWireInterface< T_WIRE >
- write() : ace_wire::SimpleWireFastInterface< T_DATA_PIN, T_CLOCK_PIN, T_DELAY_MICROS > , ace_wire::SimpleWireInterface , ace_wire::TwoWireInterface< T_WIRE >