| MD_MAX72xx LED Matrix Arduino Library 3.2.2 Library to control connected MAX72XX devices as a pixel array

Software Library

## The Library

The library implements functions that allow the MAX72xx to be used for LED matrices (64 individual LEDs), allowing the programmer to use the LED matrix as a pixel device, displaying graphics elements much like any other pixel addressable display.

In this scenario, it is convenient to abstract out the concept of the hardware device and create a uniform and consistent pixel address space, with the libraries determining device and device-element address. Similarly, control of the devices should be uniform and abstracted to a system level.

The library still retains flexibility for device level control, should the developer require, through the use of overloaded class methods.

## Conditional Compilation Switches

The library allows the run time code to be tailored through the use of compilation switches. The compile options start with USE_ and are documented in the section related to the main header file MD_MAX72xx.h.

NOTE: Compile switches must be edited in the library header file. Arduino header file 'mashing' during compilation makes the setting of these switches from user code completely unreliable.