AceWire 0.3.2 Unified interface for selecting different I2C implementations on Arduino platforms

ace_wire::SimpleWireInterface Member List

This is the complete list of members for ace_wire::SimpleWireInterface, including all inherited members.

begin() const | ace_wire::SimpleWireInterface | inline
beginTransmission(uint8_t addr) const | ace_wire::SimpleWireInterface | inline
end() const | ace_wire::SimpleWireInterface | inline
endTransmission(bool sendStop=true) const | ace_wire::SimpleWireInterface | inline
operator=(const SimpleWireInterface &)=default (defined in ace_wire::SimpleWireInterface) | ace_wire::SimpleWireInterface |
read() | ace_wire::SimpleWireInterface | inline
requestFrom(uint8_t addr, uint8_t quantity, bool sendStop=true) | ace_wire::SimpleWireInterface | inline
SimpleWireInterface(uint8_t dataPin, uint8_t clockPin, uint8_t delayMicros) | ace_wire::SimpleWireInterface | inline explicit
SimpleWireInterface(const SimpleWireInterface &)=default (defined in ace_wire::SimpleWireInterface) | ace_wire::SimpleWireInterface |
write(uint8_t data) const | ace_wire::SimpleWireInterface | inline