## ESP_DoubleResetDetector

[![arduino-library-badge](https://www.ardu-badge.com/badge/ESP_DoubleResetDetector.svg?)](https://www.ardu-badge.com/ESP_DoubleResetDetector)
[![GitHub release](https://img.shields.io/github/release/khoih-prog/ESP_DoubleResetDetector.svg)](https://github.com/khoih-prog/ESP_DoubleResetDetector/releases)
[![GitHub](https://img.shields.io/github/license/mashape/apistatus.svg)](https://github.com/khoih-prog/ESP_DoubleResetDetector/blob/master/LICENSE)
[![contributions welcome](https://img.shields.io/badge/contributions-welcome-brightgreen.svg?style=flat)](#Contributing)
[![GitHub issues](https://img.shields.io/github/issues/khoih-prog/ESP_DoubleResetDetector.svg)](http://github.com/khoih-prog/ESP_DoubleResetDetector/issues)

---
---

## Table of Contents

* [Changelog](#changelog)
  * [Releases v1.1.2](#releases-v112)
  * [Releases v1.1.1](#releases-v111)
  * [Releases v1.1.0](#releases-v110)
  * [Releases v1.0.3](#releases-v103)
  * [Releases v1.0.2](#releases-v102)
  * [Releases v1.0.1](#releases-v101)
 
---
---

## Changelog

### Releases v1.1.2

1. Update `platform.ini` and `library.json` to use original `khoih-prog` instead of `khoih.prog` after PIO fix

### Releases v1.1.1

1. Clean-up all compiler warnings possible.
2. Add Table of Contents
3. Modify Version String

### Releases v1.1.0

1. Add support to LittleFS for ESP32 using [LITTLEFS](https://github.com/lorol/LITTLEFS) Library

### Releases v1.0.3

1. Update to use the new LittleFS for ESP8266 core 2.7.1+
2. Update [minimal example](examples/minimal)

#### Releases v1.0.2

1. Fix bug by left-over cpp file.
2. Fix bug in example.
3. Enhance README.md

#### Releases v1.0.1

1. Add EEPROM and SPIFFS support, besides RTC memory, for ESP8266
2. Add SPIFFS support, besides EEPROM, for ESP32

